**TriCaster**® **TC410 Plus**

Modern producers, publishers, and content creators don’t have to disrupt the workflows they know and trust, or spend a fortune on new equipment and infrastructure to adapt to the changing media landscape. With NewTek TriCaster TC410 Plus they can push forward with confidence, taking advantage of the industry’s leading software-driven production technology, modern networking, and hundreds of future-ready capabilities to produce more incredible content for more diverse destinations, while maintaining their proven workflows and leveraging their existing investments.

TriCaster solutions are known for being complete, capable, and cost-effective for producing and delivering media content. No other integrated system provides a more complete, professional workflow for mid-range mobile and studio productions for the price.

* **Complete Production**

Produce amazing content with hundreds of advanced production capabilities for video switching, playback, mix effects, graphics, audio mixing, virtual sets, and more.

* **Format Flexibility**

Deliver an immersive viewing experience for programs, performances, events, and sports intermixing formats up to 3G 1080p resolution at 60 frames per second.

* **Native IP Processing**

NDI® video, audio and data transmission over IP with near-zero latency and instant access to and seamless interchange with essentially unlimited IP sources from anywhere across the network in real time. Integrates with products from hundreds of manufacturers and developers.

* **Multi-Source Video Mixing**

Create compelling content using any combination of 8 external compatible SDI and IP video sources, including local and remote cameras, mobile devices, Skype video calls, computers, streaming media, audio/video files, graphics, and more.

* **Multi-Destination Delivery**

Produce digital media content in various aspect ratios, resolutions, and frame rates for any screen or schedule, with 2 pairs of SDI and IP live outputs, multi-channel recording, multi-platform live streaming, social media publishing, transfer to storage volumes or network locations, and more.

* **Recording and Replay**

Record 8 channels of full-resolution video to NDI®, QuickTime® or H.264 files. Archive the master cut, ingest raw camera footage for post-production, cache production extras and presentation materials for on-demand, and capture real-time highlights for instant replay.

* **Control and Automation**

Configure custom user interfaces accessible through any Web browser or OS that deliver exactly the tools and functions needed with LivePanel™ . A comprehensive macro automation system automates settings and supports custom command sequences. Integrate production automation with Live Story Creator to run entire shows from formatted Microsoft Word scripts.

* **Live Sound Experience**

A software-based audio mixer, support for digital, analog and network audio, Talk Back communication, and 4 x 4 x 4 channel routing to four audio mix outputs.